#
RELAY INSPECTION

BME092167730W02

## Relay Type

Terminal type | Part name
--- | ---
Four-terminal | Type A | • Main relay • PCM control relay • Fuel pump relay • A/C relay • Front blower relay
• Front fog light relay
• TNS relay
• Headlight relay
• Horn relay
• Starter relay
• Headlight cleaner relay
• Rear fog light relay
Type B | • Cooling fan relay • Rear window defroster relay • Glow plug relay
Type C | • Rear blower relay
Type D | • Theft-deterrent horn relay

## Four-terminal

### Type A

1. Inspect for continuity between the relay terminals using an ohmmeter.

  • If not as specified, replace the relay.

### Type B

1. Inspect for continuity between the relay terminals using an ohmmeter.

  • If not as specified, replace the relay.

### Type C

1. Inspect for continuity between the relay terminals using an ohmmeter.

  • If not as specified, replace the relay.

### Type D

1. Inspect for continuity between the relay terminals using an ohmmeter.

  • If not as specified, replace the relay.