#
NO.3 WILL NOT CRANK [L3]

BME010300000W05

3 | WILL NOT CRANK
--- | ---
DESCRIPTION | Starter does not work.
POSSIBLE CAUSE | • Open starter circuit between ignition switch and starter • Low or dead battery. • Charging system malfunction. • Starter interlock switch malfunction (with starter interlock system). • Starter malfunction
• Seized/hydrolocked engine, flywheel

Diagnostic procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---
1 | Inspect following: • Battery connection • Battery condition • Clutch is fully depressed. (with starter interlock system) • Fuses
Are all items okay?
Yes
Go to next step.
No | Service as necessary. Repeat Step 1.
2 | Is clicking sound heard from starter when ignition switch is turned to START? | Yes | Go to next step.
No | Go to Step 4.
3 | Inspect starting system. (See STARTER INSPECTION [L3].) Is starting system okay? | Yes | Inspect for seized/hydrolocked engine, flywheel. (See FLYWHEEL INSPECTION.)
No | Repair or replace components as required.
4 | Do any other electrical accessories work? | Yes | Go to next step.
No | Inspect charging system. (See BATTERY INSPECTION.) (See GENERATOR INSPECTION [L3].)
5 | Connect WDS or equivalent to DLC-2. Retrieve any continuous memory DTCs. Are there any continuous memory DTCs displayed? | Yes | DTC is displayed: Go to appropriate DTC test. Communication error message is displayed: Inspect for following: • Open circuit between main relay and PCM terminal 2Y
• Open circuit between main relay terminal E and PCM terminal 2X
• Main relay is stuck open.
• Open or poor GND circuit (PCM terminal 4X, 2AB or 2AC)
• Poor connection of vehicle body GND
No | No DTC is displayed: Inspect following: • START circuit in ignition switch • Open circuit between ignition switch and starter • Starter interlock switch (with stater interlock system)
6 | Retrieve any KOEO DTCs. Are there DTCs displayed during KOEO inspection? | Yes | DTC is displayed: Go to appropriate DTC test.
No | No DTC is displayed: Inspect following: • START circuit in ignition switch • Open circuit between ignition switch and starter • Starter interlock switch (with stater interlock system)
7 | Verify test results. • If okay, return to diagnostic index to service any additional symptoms. • If malfunction remains, replace PCM.