#
WINDSHIELD WIPER MOTOR REMOVAL/INSTALLATION

BME091967340W01

1. Disconnect the negative battery cable.

2. Remove the windshield wiper arm and blade.

3. Remove the cowl grille.

4. Pry off the connection between the windshield wiper motor and windshield wiper link.

5. Remove in the order indicated in the table.

1 | Connector
2 | Bolt
3 | Windshield wiper motor
4 | Nut
5 | Hose
6 | Bolt
7 | Link and frame

6. Install in the reverse order of removal.

7. Adjust the windshield wiper arm and blade.