#
REAR WHEEL ALIGNMENT

BME021101016201

## Specification (Unloaded)*1

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Total toe-in | (mm {in}) | Tire : 3±4 {0.12±0.16}, Rim inner : 2±3 {0.08±0.12}
degree | 0°17'±0°22'
Camber angle (reference value) | -1°±1°

  *1 :
Engine coolant and engine oil are at specified level. Spare tire, jack and tools are in designated position.

## Rear Wheel Alignment Adjustment

1. If rear wheel alignment is not within specification, inspect for the body and torsion beam axle damage. Repair or replace if necessary.

  Note

  • Rear wheel alignment is not adjustable.