#
INTERMITTENT REAR WIPER RELAY INSPECTION

BME091966810202

1. Measure the voltage at the intermittent rear wiper relay terminals as indicated below.

2. Disconnect the intermittent rear wiper relay connector before inspecting for continuity at the terminal H.

  • If not as specified, inspect the parts listed under "Action."
  • If the parts and wiring harnesses are okay but the system still does not work properly, replace the intermittent rear wiper relay.

## Terminal Voltage Table (Reference)

Terminal | Signal | Connected to | Test condition | Voltage (V)/Continuity | Action
--- | --- | --- | --- | --- | ---
B | IG 2 | R. WIP 10 A fuse | Ignition switch at ON position | B+ | • Inspect R. WIP 10 A fuse • Inspect related harness
Other | 0
F | Rear wiper switch INT | Rear wiper switch | Ignition switch at ON position | Rear wiper switch at INT position | 0 | • Inspect R. WIP 10 A fuse • Inspect wiper and washer switch (See WIPER AND WASHER SWITCH INSPECTION.) • Inspect related harness
• Rear wiper switch at OFF position • Rear wiper switch at ON position | B+
H | GND | GND | Under any condition: inspect for continuity to ground | Yes | • Inspect GND • Inspect related harness
J | Autostop | Rear wiper motor | Rear wiper is operating (INT position or ON position) | Alternates 0 and B+ | • Inspect R. WIP 10 A fuse • Inspect wiper and washer switch (See WIPER AND WASHER SWITCH INSPECTION.) • Inspect rear wiper motor (See REAR WIPER MOTOR INSPECTION.)
• Inspect related harness
Other | B+