#
ON-BOARD DIAGNOSTIC SYSTEM PID/DATA MONITOR FUNCTION

BME040267650T03

PID/DATA Monitor Table

PID name | input/output part | Operation/unit
--- | --- | ---
ABS_LAMP | ABS warning light driver output state | ON/OFF
ABSLF_ I | LF ABS pressure retention valve output state | ON/OFF
ABSLF_O | LF ABS pressure reduction valve output state | ON/OFF
ABSLR_I | LR ABS pressure retention valve output state | ON/OFF
ABSLR_O | LR ABS pressure reduction valve output state | ON/OFF
ABSRF_I | RF ABS pressure retention valve output state | ON/OFF
ABSRF_O | RF ABS pressure reduction valve output state | ON/OFF
ABSRR_I | RR ABS pressure retention valve output state | ON/OFF
ABSRR_O | RR ABS pressure reduction valve output state | ON/OFF
BOO_ABS | Brake pedal switch input | ON/OFF
BRAKE_LMP | BRAKE system warning light driver output state | ON/OFF
LF_WSPD | LF wheel-speed sensor input | KPH/MPH
LR_WSPD | LR wheel-speed sensor input | KPH/MPH
ABSPMPRLY | ABS motor relay output state | ON/OFF
PMP_MOTOR | ABS motor output state | ON/OFF
RF_WSPD | RF wheel-speed sensor input | KPH/MPH
RR_WSPD | RR wheel-speed sensor input | KPH/MPH
ABSVLVRLY | Fail-safe relay output state | ON/OFF
RPM* | Engine speed | RPM
TRAC_SW* | TCS OFF switch | ON/OFF
ABS_VOLT | System battery voltage value | V

  *:
With TCS