#
DTC TABLE

BME090266900W04

Screen display | Malfunction location | Page
--- | --- | ---
DTC | Output signal
09 ERR22 or 09:Er22 | - | Base unit (peripheral circuit) | (See DTC 09 ERR22 OR 09:ER22)
09 ERR20 or 09:Er20 | - | Power supply circuit of base unit | (See DTC 09 ERR20 OR 09:ER20)
00 ERR10 or 00:Er10 | - | Cassette deck-base unit communication line | (See DTC 00 ERR10 OR 00:ER10)
03 ERR10 or 03:Er10 | - | CD player-base unit communication line | (See DTC 03 ERR10 OR 03:ER10)
05 ERR10 or 05:Er10 | - | CD changer (external type)-base unit communication line | (See DTC 05 ERR10 OR 05:ER10)
06 ERR10 or 06:Er10 | - | CD changer (upper module)-base unit communication line | (See DTC 06 ERR10 OR 06:ER10)
07 ERR10 or 07:Er10 | - | MD player-base unit communication line | (See DTC 07 ERR10 OR 07:ER10)
03 ERR01 or 03:Er01 | - | CD player | (See DTC 03 ERR01 OR 03:ER01)
03 ERR02 or 03:Er02 | CHECK*1 CD*2 | CD player | (See DTC 03 ERR02 OR 03:ER02)
03 ERR07 or 03:Er07 | CHECK*1 CD*2 | CD player | (See DTC 03 ERR07 OR 03:ER07)
00 ERR01 or 00:Er01 | - | Cassette deck | (See DTC 00 ERR01 OR 00:ER01)
00 ERR03 or 00:Er03 | - | Cassette deck | (See DTC 00 ERR03 OR 00:ER03)
00 ERR04 or 00:Er04 | CHECK*1 TAPE*2 | Cassette tape | (See DTC 00 ERR04 OR 00:ER04)
05 ERR01 or 05:Er01 | - | CD changer (external type) | (See DTC 05 ERR01 OR 05:ER01)
05 ERR07 or 05:Er07 | CHECK*1 CD*2 | CD changer (external type) | (See DTC 05 ERR07 OR 05:ER07)
06 ERR01 or 06:Er01 | - | CD changer (upper module) | (See DTC 06 ERR01 OR 06:ER01)
06 ERR02 or 06:Er02 | CHECK*1 CD*2 | CD changer (upper module) | (See DTC 06 ERR02 OR 06:ER02)
06 ERR07 or 06:Er07 | CHECK*1 CD*2 | CD changer (upper module) | (See DTC 06 ERR07 OR 06:ER07)
07 ERR01 or 07:Er01 | - | MD player | (See DTC 07 ERR01 OR 07:ER01)
07 ERR02 or 07:Er02 | CHECK*1 MD*2 | MD player | (See DTC 07 ERR02 OR 07:ER02)
07 ERR07 or 07:Er07 | CHECK*1 MD*2 | MD player | (See DTC 07 ERR07 OR 07:ER07)
NO ERR or no Err | - | No stored DTCs | -

  *1,*2 :
When an error occurs, the error messages are displayed three times in the order of *1 and *2, respectively.