#
TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5A-EL]

BME051719440201

  Note

  • Input signals of the TR switch can be inspected with a WDS or equivalent. (See TCM INSPECTION [JA5A-EL] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513).) (See TCM INSPECTION [JA5A-EL] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).)

## Operation Inspection

1. Verify that the starter operates only with the ignition switch is turned to the START position with the selector lever in P or N positions.

  • If there is any malfunction, inspect for continuity at the TR switch. (See Continuity Inspection.)

2. Verify that the back-up lights illuminate when shifted to R position with the ignition switch at the ON position.

  • If there is any malfunction, inspect for continuity at the TR switch.

## Continuity Inspection

1. Disconnect the TR switch connector.

2. Verify that the continuity is as indicated in the table.

  • If there is any malfunction, adjust the TR switch, then reinspect the TR switch. (See TRANSAXLE RANGE (TR) SWITCH ADJUSTMENT [JA5A-EL].)

3. Connect the TR switch connector.