#
SLIDING DOOR DISASSEMBLY/ASSEMBLY

BME091173002202

1. Lower or raise the rear door glass so that the distance from the top of the rear door glass at the rear end to the upper part of the rear beltline molding is 260 mm {10 in}.

2. Disconnect the negative battery cable.

3. Remove the sliding door trim. (See SLIDING DOOR TRIM REMOVAL/INSTALLATION.)

4. To remove the rear door glass, remove the rear beltline molding. (SeeREAR BELTLINE MOLDING REMOVAL/INSTALLATION.)

5. Disassemble in the order indicated in the table.

6. Assemble in the reverse order of disassembly.

1 | Door screen
2 | Door lock knob
3 | Glass guide
4 | Rear door glass (See Rear Door Glass Disassembly Note)
5 | Glass run channel
6 | Rear power window regulator
7 | Remote controller
8 | Rear door lock
9 | Outer handle
10 | Sliding door circuit contact
11 | Sliding door circuit contact (with PSD system)
12 | Upper roller
13 | Center roller
14 | Open lock actuator (except with PSD system)
15 | Lower roller
16 | Easy closure control module (with PSD system)

## Rear Door Glass Disassembly Note

1. Remove the rear door glass installation bolts.

2. To remove the rear door glass from the glass run channel, lower the rear door glass.

3. Lift the rear door glass out of the sliding door.