#
FRONT DOOR LOCK ACTUATOR REMOVAL/INSTALLATION

BME091458310201

1. Fully raise the front door glass.

2. Disconnect the negative battery cable.

3. Remove the door screen.

4. Disconnect the front door lock actuator connector.

5. Disconnect the rods and the cables.

6. Remove the screws and the front door lock.

7. Remove the screws, and remove the front door lock actuator from the front door lock.

8. Install in the reverse order of removal.