#
DTC P0225 [MZR-CD (RF Turbo)]

BME010200102269

DTC P0225 | Idle switch circuit malfunction
--- | ---
DETECTION CONDITION | • The PCM monitors the input signals from the accelerator pedal position sensor and the idle switch. If the idle switch is off even if the voltage from the accelerator pedal position sensor is less than 0.75 V, the PCM determines that there is a malfunction in the idle switch circuit. Diagnostic support note
• The MIL illuminates if the PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM.
• PENDING CODE is available if PCM detects the above malfunction condition during the first drive cycle.
• FREEZE FRAME DATA is available.
• DTC is stored in the PCM memory.
POSSIBLE CAUSE | • Idle switch malfunction • Connector or terminal malfunction • Open circuit in wiring harness between idle switch terminal B and GND • Open circuit in wiring harness between idle switch terminal A and PCM terminal 31 • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY CURRENT SIGNAL STATUS: IS CONCERN INTERMITTENT OR CONSTANT? • Connect the WDS or equivalent to the DLC-2. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the PENDING CODE for this DTC present? | Yes | Go to the next step.
No | Intermittent concern exists. Perform the "INTERMITTENT CONCERN TROUBLESHOOTING". (See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)].)
4 | INSPECT IDLE SWITCH CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Inspect for poor connection (such as damaged/pulled-out terminals, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 9.
No | Go to the next step.
5 | INSPECT IDLE SWITCH GND CIRCUIT FOR OPEN CIRCUIT • Turn the engine switch off. • Inspect for continuity between idle switch terminal B and body GND. • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for an open circuit, then go to Step 9.
6 | INSPECT IDLE SWITCH • Inspect the idle switch. (See IDLE SWITCH INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace the accelerator pedal component, then go to Step 9.
No | Go to the next step.
7 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Inspect for poor connection (such as damaged/pulled-out terminals, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 9.
No | Go to the next step.
8 | INSPECT IDLE SWITCH SIGNAL CIRCUIT FOR OPEN CIRCUIT • Turn the engine switch off. • Inspect for continuity between idle switch terminal A and PCM terminal 31. • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for an open circuit, then go to the next step.
9 | VERIFY TROUBLESHOOTING OF DTC P0225 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the PENDING CODE for this DTC present? | Yes | Replace the PCM, then go to the next step.
No | Go to the next step.
10 | VERIFY AFTER REPAIR PROCEDURE • Perform the Repair Verification Drive Mode. (See OBD DRIVE MODE [MZR-CD (RF Turbo)].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | Troubleshooting completed.