#
RUNNING LIGHT UNIT REMOVAL/INSTALLATION

BME091866731201

  Note

  • Because the lock section of the unit is damaged easily, do not remove the unit from the bracket unless replacement is necessary. Always perform an inspection of the running light unit before removal.

1. Disconnect the negative battery cable.

2. Remove the bracket.

3. Disconnect the running light unit connector.

4. Remove the running light unit by prying the lock section of the side part with a flathead screwdriver.

5. Install in the reverse order of removal.