#
DTC C1510 (32), C1511 (33), C1512 (34), C1513 (35)

BME040243000207

DTC | C1510 (32) C1511 (33) C1512 (34) C1513 (35) | RF solenoid valve, ABS motor or RF ABS wheel-speed sensor/sensor rotor. LF solenoid valve, ABS motor or LF ABS wheel-speed sensor/sensor rotor. RR solenoid valve, ABS motor or RR ABS wheel-speed sensor/sensor rotor. LR solenoid valve, ABS motor or LR ABS wheel-speed sensor/sensor rotor.
DETECTION CONDITION | • Wheel lock is detected during ABS operation (pressure reduction inoperative).
POSSIBLE CAUSE | • Low electrical power supply • Malfunction of solenoid valve in ABS/TCS HU/CM or ABS HU/CM • Malfunction of ABS wheel-speed sensor • Damaged ABS sensor rotor • Stuck ABS motor in ABS/TCS HU/CM or ABS HU/CM
• Malfunction of hydraulic unit of ABS/TCS HU/CM or ABS HU/CM

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY OTHER DTC HAS BEEN RECORDED • Is DTC B1318 (63) also stored? | Yes | Go to DTC B1318 (63) inspection.
No | Go to next step.
2 | VERIFY OTHER DTC HAS BEEN RECORDED • Are any of DTC C1214 (22), C1210 (23), C1198 (24), C1194 (25), C1254 (26), C1246 (27), C1250 (28) and/or C1242 (29) also stored? | Yes | Go to applicable DTC inspection.
No | Go to next step.
3 | VERIFY OTHER DTC HAS BEEN RECORDED • Are any of DTC C1145 (11), C1148 (41), C1155 (12) C1158 (42), C1165 (13), C1168 (43), C1175 (14), C1178 (44), C1233 (46), C1234 (45), C1235 (47) and/or C1236 (48) also stored? | Yes | Go to applicable DTC inspection.
No | Go to next step.
4 | VERIFY OTHER DTC HAS RECORDED • Is any of DTC C1095 (54) an/or C1096 (53) also memorized? | Yes | Go to applicable DTC inspection.
No | Go to next step.
5 | INSPECT ABS/TCS HU/CM or ABS HU/CM OPERATION • Perform ABS/TCS HU/CM or ABS HU/CM system inspection. (See ABS HU/CM REMOVAL/INSTALLATION) (See ABS/TCS HU/CM REMOVAL/INSTALLATION) • Is it okay? | Yes | Go to next step.
No | Replace ABS/TCS HU/CM or ABS HU/CM, then go to next step.
6 | VERIFY CURRENT STATUS OF MALFUNCTION • Clear DTC from memory. (See Clearing DTCs Procedure) • Start engine and drive vehicle at 10 km/h {6.2 mph} or above at least one minute. • Gradually slow down and stop vehicle.
• Is same DTC present?
Yes
Replace ABS/TCS HU/CM or ABS HU/CM.
No | Go to next step.
7 | VERIFY AFTER REPAIR PROCEDURE • Is there any other DTC present? | Yes | Go to applicable DTC inspection.
No | Troubleshooting completed.