#
WHEEL APRON PANEL (FRONT) AND APRON REINFORCEMENT REMOVAL

BME098053211B01

1. After removing the cowl side reinforcement, remove the apron reinforcement and wheel apron panel (front).

2. When removing the wheel apron panel (front) and apron reinforcement at the same time, it is not necessary to drill the 15 weld locations sections marked (A).

  Note

  • The plug welds marked (B) indicate the same section.

3. After drilling each section, remove by pulling forward.

4. The hinge pillar inner is covered in sections marked (C); the weld locations cannot be checked. Bend the hinge pillar inner outward before drilling.