#
REASSEMBLY

A6E201400004E11

• Standard values, such as torques and certain adjustments, must be strictly observed in the reassembly of all parts.

• If removed, these parts should be replaced with new ones:

  - Oil seals
  - Gaskets
  - O-rings
  - Lockwashers
  - Cotter pins
  - Nylon nuts

• Depending on location:

  - Sealant and gaskets, or both, should be applied to specified locations. When sealant is applied, parts should be installed before sealant hardens to prevent leakage.
  - Oil should be applied to the moving components of parts.
  - Specified oil or grease should be applied at the prescribed locations (such as oil seals) before reassembly.