#
ENGINE DISASSEMBLY/ASSEMBLY [L3]

BME011001001204

1. Disconnect the engine and transaxle. (See MANUAL TRANSAXLE REMOVAL/INSTALLATION [G15M-R].)

2. Remove the Clutch unit. (See CLUTCH UNIT REMOVAL/INSTALLATION.)

3. Remove the intake-air system. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L3].)

4. Remove the exhaust system. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L3].)

5. Remove the generator. (See GENERATOR REMOVAL/INSTALLATION [L3].)

6. Remove the ignition coils. (See IGNITION COIL REMOVAL/INSTALLATION [L3].)

7. Remove the Crankshaft position sensor. (See CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION [L3].)

8. No.2 engine mount bracket.

9. Assemble in the reverse order of disassembly.