#
ENGINE SPECIFICATIONS

BME010002000103

Lubrication system

Item | Specification
--- | ---
L3 | AJ | MZR-CD (RF Turbo)
Lubrication system | Force-fed type
Oil cooler (with oil cooler) | Water-cooled
Oil pressure (reference value) | 300-549 {3.1-5.6, 44-80} [3,000] | 138-310 {1.4-3.2, 20-45} [1,500] | Minimum 147 {1.5, 21} [1,000] Minimum 343 {3.5, 50} [3,000]
(kPa {kgf/cm2, psi} [rpm])
Oil pump | Type | Trochoid gear type
Relief pressure (reference value) | 500-600 {5.09-6.11, 72.6-87.0} | - | 580-700 {5.9-7.1, 84.1-101.5} [3,000]
(kPa {kgf/cm2, psi})
Oil filter | Type | Full-flow, paper element
Bypass pressure (reference value) | 80-120 {0.9-1.2, 12.8-17.0} | - | 78-118 {0.8-1.2, 11.3-17.1}
(kPa kgf/cm2, psi})
Oil capacity (Approx. quantity) | Total (Dry engine) | 5.1 {5.4, 4.5} | 6.2 {6.6, 5.5} | 5.5 {5.8, 4.8}
(L {US qt, lmp qt})
Oil replacement | 4.0 {4.2, 3.5} | 5.2 {5.5, 4.6} | 4.8 {5.1, 4.2}
(L {US qt, lmp qt})
Oil and oil filter replacement | 4.4 {4.6, 3.9} | 5.7 {6.0, 5.0} | 5.0 {5.3 ,4.4}
(L {US qt, lmp qt})

Recommended Engine Oil

Item | Specification
--- | ---
Gasoline engine, Europe | Diesel engine, Europe | Except Europe
Engine oil | Grade | API | SL | CF | CF | CD, CE, CF-4 | SH, SJ, SL
ILSAC | - | - | - | - | GF-2, GF-3
ACEA | A3, A5 | A3 | B1, B3, B5 | B3 | B3, B4 | -
Viscosity (SAE) | 5W-30 | 10W-40 | 5W-20 | 5W-30 | 10W-40 | 5W-30, 10W-30 | 5W-20, 5W-30, 10W-30
Remarks | Mazda genuine Dexelia oil e.g. | - | Mazda genuine Dexelia oil e.g. | - | -