#
WATER PUMP REMOVAL/INSTALLATION [L3]

BME011215010W01

1. Disconnect the negative battery cable.

2. Drain the engine coolant. (See COOLING SYSTEM SERVICE WARNINGS.)(See ENGINE COOLANT REPLACEMENT [L3].)

3. Loosen the water pump pulley bolt and remove the drive belt. (See DRIVE BELT REPLACEMENT [L3].)

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. Inspect the drive belt. (See DRIVE BELT INSPECTION [L3].)

7. Refill the engine coolant. (See ENGINE COOLANT REPLACEMENT [L3].)

1 | Water pump pulley
2 | Water pump
3 | O-ring