#
COOLING FAN MOTOR INSPECTION

BME011215025W01

1. Verify that the battery is fully charged. (See Battery.)

2. Disconnect the fan control module connector.

3. Connect the battery voltage and an ammeter to the fan control module connector on fan motor side.

4. Perform the same procedure as Step 2 for the condenser fan motor.

5. Verify that the cooling fan motor operates smoothly at the standard current draw.

  • If not within the specification, replace the cooling fan motor.

Item | Current (A)
--- | ---
Cooling fan | 4.3-7.3
Condenser fan | 8.5-11.5