#
FRONT FOG LIGHT REMOVAL/INSTALLATION

BME091851680202

1. Disconnect the negative battery cable.

2. Remove the mud guard.

3. Remove in the order indicated in the table.

Standard

Sports

1 | Connector
2 | Screw
3 | Screw
4 | Bolt (Sports)
5 | Bracket (Standard)
6 | Front fog light cover (Sports)
7 | Front fog light

4. Install in the reverse order of removal.

5. Adjust the front fog light aiming. (See FRONT FOG LIGHT AIMING.)