#
DTC 06 ERR01 OR 06:ER01

BME090266900220

DTC 06 ERR01 or 06:Er01 | CD changer (upper module)
DETECTION CONDITION | • CD changer (upper module) cannot implement insert, eject, and disc change commands.
POSSIBLE CAUSE | • Defective CD (broken or foreign material stuck/attached) • CD changer (upper module) malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Is CD able to be ejected? | Yes | Go to next step.
No | Replace CD changer (upper module).
2 | INSPECT CD • Inspect condition of CD where error has occurred. • Is CD okay? | Yes | Go to next step.
No | Repair (remove foreign material) or replace CD, then go to next step.
3 | INSPECT CD CHANGER (UPPER MODULE) • Clear DTC. • Insert and eject CD with no defect. • Start on-board diagnostic test mode. • Is DTC 06 ERR01 or 06:Er01 displayed? | Yes | Replace CD changer (upper module).
No | Troubleshooting completed.