#
ABS/TCS HU/CM REMOVAL/INSTALLATION

BME041467650201

  Caution

  • Do not drop the ABS/TCS HU/CM. Replace it if it is subjected to an impact.

1. Remove the splash shield.

2. Remove the battery.

3. Remove the air cleaner. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L3].) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [AJ].) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

4. For the MZR-CD (RF-Turbo) engine model, remove the fuel filter installation bolt and put the fuel filter aside. (See FUEL FILTER COMPONENT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

1 | Brake pipe (See Brake Pipe Removal Note) (See Brake Pipe Installation Note)
2 | Connector (See Connector Removal Note) (See Connector Installation Note)
3 | ABS/TCS HU/CM (See ABS/TCS HU/CM Removal/Installation Note)
4 | Stud

## Connector Removal Note

1. Pull the lock lever up and make it unlock.

2. Remove the connector.

## Brake Pipe Removal Note

1. Mark the brake pipe connecting positions before removal for reference during installation.

## ABS/TCS HU/CM Removal/Installation Note

1. When removing/installing the ABS/TCS HU/CM from/to the vehicle, attach a strip of protective tape on the ABS/TCS HU/CM connector to prevent brake fluid from entering.

## Brake Pipe Installation Note

1. When installing the brake pipe, align the marks made before removal with the ABS/TCS HU/CM as shown in the figure.

## Connector Installation Note

1. Verify that the lock lever of the harness connector is completely pulled up.