#
CHECK POWER SLIDING DOOR (PSD) SYSTEM OPERATION

BME090373001205

  Note

  • The buzzer that warns of abnormality stops when main switch is turned from ON position to OFF position.

Vehicle condition | Door condition | Check procedure | Normal condition
--- | --- | --- | ---
• Main switch is at ON position. • Door lock knob is in unlock position. • IG switch is in OFF or ACC position. • Selector lever is in P position. | Fully closed | • Press PSD front OPEN switch. • Press PSD rear switch. • Press transmitter R/L button. • Manually open sliding door approx. 50 mm {1.97 in}. | • Buzzer sounds once and door opens fully. • Interior light and door ajar warning light illuminate when the door is opened.
Fully open | • Press PSD front CLOSE switch. • Press the PSD rear switch. • Press the transmitter R/L button. • Manually close the sliding door approx. 100 mm {3.94 in}. | Buzzer sounds once and door closes fully.
During close operation | Press any of the following: • PSD front OPEN switch • PSD front CLOSE switch • PSD rear switch • Transmitter R/L button | Buzzer sounds once and door stops at the position.
After the sliding door is stopped by switch operation during close operation. | Manually push the sliding door in open direction until it stops, then slide it in close direction. | • Door can be manually closed to ajar. • Door automatically closes from door ajar position.
Partly open | Press PSD front CLOSE switch. | Buzzer sounds once and door closes fully.
Partly open | Press any of the following: • PSD front OPEN switch • PSD rear switch • Transmitter R/L button | Buzzer sounds once and door opens fully.
• Main switch is at ON position. • Door lock knob is in lock position. • IG switch is in OFF or ACC position. • Selector lever is in P position. | Fully closed | Press any of the following: • PSD front OPEN switch • PSD rear switch • Transmitter R/L button | Buzzer sounds once and the door does not open. (No operation sound)
• Main switch is at ON position. • Door lock knob is in unlock position. • IG switch is in ON position. • Selector lever is in N position. • Brake pedal is not depressed and the parking brake lever is released. | Fully closed | Press any of the following: • PSD front OPEN switch • PSD rear switch • Transmitter R/L button | Buzzer sounds once and door opens fully.
• Main switch is at ON position. • Door lock knob is in unlock position. • IG switch is in ON position. • Selector lever is in P position. • Brake pedal is depressed. (Brake switch is off.)
• Parking brake lever is released. (Parking brake switch is off.)
During close operation
Shift the selector lever from P position to other position
Buzzer sounds once when the door is closed.
During open operation | Shift the selector lever from P position to other position | • Sliding door stops. • Buzzer sounds continuously. (The buzzer stops when the main switch is turned from out-position to in-position.
Main switch is at OFF position. | Fully closed (After automatically closed) | Manually open the sliding door. | Door can be manually opened to fully open position.
Fully open (After automatically opened) | Manually close the sliding door. | • Door can be manually closed to ajar. • Door automatically closes from door ajar position.
• Main switch is at ON position. • Door lock knob is in unlock position. • IG switch is in OFF or ACC position. • Selector lever is in P position. • Child safety lock lever is at LOCK position. | Fully closed | • Press PSD front OPEN switch. • Press transmitter R/L button. • Manually open the sliding door by the outer handle. | • Buzzer sounds once and the door opens fully. • Interior light and the door ajar warning light illuminate when the door is opened.
• Press the PSD rear switch. • Manually open the sliding door by the inner handle. | • Buzzer does not sound. • Door does not open.