#
SHIFT-LOCK RELAY INSPECTION

BME051830000204

1. Disconnect the negative battery cable.

2. Disconnect the shift-lock relay connector.

3. Inspect voltage and continuity between the shift-lock relay terminals.

  • If there is any malfunction, replace the shift-lock relay. (See SHIFT-LOCK RELAY REMOVAL/INSTALLATION.)

4. Connect the shift-lock relay connector.

5. Connect the negative battery cable.