#
AUTOMATIC TRANSAXLE [FN4A-EL] SPECIFICATIONS

BME050001024103

Item | Specifications
--- | ---
Engine type | L3
Gear ratio | 1GR | 2.816
2GR | 1.553
3GR | 1.000
4GR | 0.695
Reverse | 2.279
Final gear ratio | 4.416
ATF | Type | ATF M-V
Capacity (Approx. quantity) | 7.8 {8.2, 6.9}
(L {US qt, lmp qt})
Torque converter stall torque ratio | 1.78
Hydraulic system (Number of drive/driven gear plates) | Forward clutch | 4/4
3-4 clutch | 3/3
Reverse clutch | 2/2
Low and reverse brake | 5/5
Band servo | Servo diameter (Piston outer dia.) | 64.6 {2.54}
(mm {in})
Front planetary gear (Number of teeth) | Front sun gear | 49
Front pinion gear | 20
Front internal gear | 89
Rear planetary gear (Number of teeth) | Rear sun gear | 43
Rear pinion gear | 27
Rear internal gear | 98
Primary gear (number of teeth) | 86
Secondary gear (number of teeth) | 82
Output gear (number of teeth) | 19
Ring gear (number of teeth) | 88