#
BASIC INSPECTION [FN4A-EL]

BME050301030202

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Perform the mechanical system test. (See MECHANICAL SYSTEM TEST [FN4A-EL].) Is the mechanical system normal? | Yes | Go to the next step.
No | Repair or replace any malfunctioning parts according to the inspection result.
2 | Turn the ignition switch to the ON position. When the selector lever is moved, dose the selector indicator light indication correspond to the lever location? Also, when other ranges are selected from N or P during idling, does the vehicle move within 1-2 s? | Yes | Go to the next step.
No | Inspect the selector lever and TR switch. Repair or replace malfunctioning parts. (See SELECTOR LEVER INSPECTION.) (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [FN4A-EL].) If the selector lever and TR switch are normal, go to the next step.
3 | Inspect the ATF color and condition. (See AUTOMATIC TRANSAXLE FLUID (ATF) INSPECTION [FN4A-EL].) Are the ATF color and ordor normal? | Yes | Go to the next step.
No | Repair or replace any malfunctioning parts according to the inspection result. Flush the ATX and cooler line if necessary.
4 | Perform the line pressure test. (See Line Pressure Test.) Is the line pressure normal? | Yes | Go to the next step.
No | Adjust the accelerator cable if necessary. Repair or replace any malfunctioning parts according to the inspection result.
5 | Perform the stall test. (See Stall Test.) Is the stall speed normal? | Yes | Go to the next step.
No | Repair or replace any malfunctioning parts according to the inspection result.
6 | Inspect the value at the following PCM PIDs using the WDS or equivalent. (See PCM INSPECTION [L3].) • TFT • TFTV • VPWR
• TR
• ECT
• TCS
• RPM
• TP
• TSS
• VSS
Are the PID values normal?
Yes
Perform the symptom troubleshooting and follow the procedures.
No | Repair or replace any malfunctioning parts according to the inspection result.