#
DIFFERENTIAL ASSEMBLY

BME051527100M03

1. Assemble in the order indicated in the table.

A65M-R

.

1 | Ring gear (See Ring Gear Assembly Note.)
2 | Gear case component
3 | Bearing (ring gear side) (See Bearing (Ring Gear Side) Assembly Note.)
4 | Spacer (See Spacer Assembly Note.)
5 | Bearing (ring gear-opposite side) (See Bearing (Ring Gear-Opposite Side) Assembly Note.)

A65MX-R

.

1 | Ring gear (See Ring Gear Assembly Note.)
2 | Gear case component
3 | Bearing (ring gear side) (See Bearing (Ring Gear Side) Assembly Note.)
4 | Reduction gear (See Reduction Gear Assembly Note.)
5 | Speedometer drive gear
6 | Spacer (See Spacer Assembly Note.)
7 | Bearing (ring gear-opposite side) (See Bearing (Ring Gear-Opposite Side) Assembly Note.)

## Ring Gear Assembly Note

1. Install the gear case component, and tighten a bolt in the order shown in the figure.

Tightening torque

  A65M-R: 112.7-127.4 N·m {11.5-13.0 kgf·m, 83-94 ft·lbf}
  A65MX-R: 120 N·m {12.2 kgf·m, 88.5 ft·lbf}

## Bearing (Ring Gear Side) Assembly Note

1. Install a new bearing using the SSTs.

A65M-R

A65MX-R

## Reduction Gear Assembly Note

1. Install the reduction gear, and tighten a bolt in the order shown in the figure.

Tightening torque

  96 N·m {9.8 kgf·m, 71 ft·lbf}

## Spacer Assembly Note

1. Install the spacer using the SST.

## Bearing (Ring Gear-Opposite Side) Assembly Note

1. Install a new bearing using the SSTs.