#
TCM REMOVAL/INSTALLATION [JA5A-EL]

BME051718901202

1. Disconnect the negative battery cable.

2. Remove the floor mat of passenger seat.

3. Disconnect the negative battery cable.

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. Install the floor mat of passenger seat.

7. Connect the negative battery cable.

1 | Flange cap nut
2 | TCM panel
3 | TCM connector
4 | TCM