#
POWER DOOR LOCK SYSTEM WIRING DIAGRAM

BME091466000T06

1 | Key reminder switch
2 | Door lock timer unit
3 | European (L.H.D. U.K.) specs. only
4 | Australian, General (L.H.D.) specs. only
5 | Front door lock actuator (driver's side)
6 | Front door lock actuator (passenger's side)
7 | Sliding door lock actuator (left side)
8 | Sliding door lock actuator (right side)
9 | Liftgate lock actuator
10 | Lock
11 | Double lock
12 | Unlock
13 | Door key cylinder switch (driver's side)
14 | Door key cylinder switch (passenger's side)
15 | Liftgate key cylinder switch
16 | U.K. specs. with theft-deterrent system only
17 | Theft-deterrent control module
18 | Door lock-link switch
19 | Instrument cluster
20 | Microcomputer
21 | Security light
22 | Keyless unit
23 | Horn relay
24 | Horn
25 | Australian, European (L.H.D. U.K.) specs.
26 | Door switch
27 | Cargo compartment light switch
28 | Without PSD
29 | Except general (R.H.D.) specs.
30 | PSD control module (LH)
31 | PSD control module (RH)
32 | With PSD
33 | Flasher unit