#
FRONT FOG LIGHT AIMING

BME091851680W03

1. Adjust the tire air pressure to the specification.

2. Position the unloaded vehicle on a flat, level surface.

3. Seat one person in the driver's seat.

4. Position the vehicle 3 m {10 ft} in front of a white screen.

5. While adjusting one fog light, mask the other.

6. Start the engine to charge the battery.

7. Turn the front fog light on.

8. Adjust the brightness border line by turning the adjusting bolts as shown in the figure. Loosen the bolts first, then tighten them.

  Note

  • If the adjusting bolts are tightened first, then loosened, they will continue to loosen when the vehicle is in motion and may cause the front fog lights to become misaligned.