#
NO.27 HOLD INDICATOR LIGHT DOES NOT ILLUMINATE WHEN HOLD SWITCH IS TURNED TO ON [FN4A-EL]

BME050301030231

27 | HOLD indicator light does not illuminate when HOLD switch is turned to ON
DESCRIPTION | • HOLD indicator light in instrument cluster does not illuminate when the HOLD switch is turned on with the ignition switch at ON.
POSSIBLE CAUSE | • HOLD switch, HOLD indicator light or related wiring harness malfunction.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Do other indicator lights illuminate with the ignition switch at ON? | Yes | Inspect the meter fuse.
No | Go to the next step.
2 | Inspect the HOLD switch. (See HOLD SWITCH INSPECTION [FN4A-EL].) Is the HOLD switch normal? | Yes | Go to the next step.
No | Repair or replace any malfunctioning parts.
3 | Disconnect the PCM connector. Turn the ignition switch to the ON position. Is the voltage between 3Q terminal at the PCM connector and the body ground more than 10.5 V? | Yes | Replace the PCM.
No | Reconnect the PCM. Go to the next step.
4 | Inspect the HOLD indicator light. Is the HOLD indicator light normal? | Yes | Inspect for open circuit or disconnected connector in harness between the following: • Ignition switch and HOLD indicator light • HOLD indicator light and PCM
No | Repair or replace any malfunctioning parts.