#
JACKING POSITIONS, VEHICLE LIFT (2 SUPPORTS) AND SAFETY STAND (RIGID RACK) POSITIONS

BME000000000W06

## Jacking Positions

  Warning

  • Improperly jacking a vehicle is dangerous. The vehicle can slip off the jack and cause serious injury. Use only the correct front and rear jacking points and block the wheels.

• Use safety stands to support the vehicle after it has been lifted.

### Front

  • At the jacking plate of the engine support member.

### Rear

  • At the center of torsion beam axle.

## Vehicle Lift Positions

### Front and rear

  Warning

  • Unstably lifting a vehicle is dangerous. The vehicle can slip off the lift and cause serious injury and/or vehicle damage. Make sure that the vehicle is on the lift horizontally by adjusting the height of support at the end of the arm of the lift.

## Safety Stand Positions

### Front

  • Both sides of the vehicle, on side sills.

### Rear

  • Both sides of the vehicle, on side sills.

Jacking positions, vehicle lift (2 supports) and safety stand (rigid rack) positions view