#
IMMOBILIZER UNIT REMOVAL/INSTALLATION

BME091467003W01

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

  Caution

  • After replacing the immobilizer unit with a new one, the engine cannot be started without reprogramming the ID number of the keys and the code word of the new immobilizer unit. Input the ID number and code word. (See IMMOBILIZER SYSTEM REPROGRAM PROCEDURE.)

1 | Connector
2 | Immobilizer unit