#
CONTROL SYSTEM STRUCTURAL VIEW [AJ]

BME014000000T53

L.H.D.

R.H.D.

1 | PCM
2 | TCM
3 | A/C switch
4 | VSS
5 | Drive information system display
6 | Water temperature gauge
7 | Generator warning light
8 | MIL
9 | Brake switch
10 | IAC valve
11 | TP sensor
12 | EGR valve
13 | BARO sensor (European (L.H.D.) specs.)/EGR boost sensor (Australian, General (L.H.D. R.H.D.) specs.)
14 | EGR boost sensor solenoid valve (used for Australian, General (L.H.D. R.H.D.) specs.)
15 | MAF/IAT sensor
16 | DLC
17 | Fuel pump relay
18 | Main relay
19 | Purge solenoid valve
20 | Battery
21 | ECT sensor
22 | TR switch
23 | Fan control module
24 | CKP sensor
25 | CMP sensor
26 | Fuel injector
27 | PSP switch
28 | Intake manifold communication control (IMCC) actuator
29 | Generator
30 | Knock sensor
31 | HO2S (front, RH)
32 | HO2S (front, LH)
33 | HO2S (rear, RH) (European (L.H.D.) specs.)
34 | HO2S (rear, LH) (European (L.H.D.) specs.)