#
ENGINE MOUNT CONSTRUCTION [AJ]

BME011039000T01
• The engine is mounted at four points (fore, aft, right, and left).
• The No.3 engine mounting rubber is oil-filled.

1 | No.1 engine mounting rubber
2 | No.1 engine mounting bracket
3 | No.2 engine mounting rubber
4 | No.2 engine mounting bracket
5 | No.3 engine mounting rubber
6 | No.3 engine joint bracket
7 | No.3 engine mounting bracket
8 | No.4 engine mounting rubber
9 | No.4 engine mounting bracket
10 | Engine mount member
11 | Engine front
12 | No.3 engine mounting rubber (cross section)
13 | Rubber
14 | Oil