#
DRIVE BELT [L3]

BME011015800T01

## Structure

• A serpentine type drive belt with a V-ribbed belt to drive the supplemental units has been adopted. This shortens the engine length and improve serviceability.
• A front drive belt auto tensioner with an embedded coil spring has been adopted to automatically maintain the optimal drive belt tension.

Drive Belt Specification.

ITEM | L3
--- | ---
Belt length size | mm {in} | About 2,305 {90.75}
Belt width size | mm {in} | About 20.5 {0.81}

1 | P/S oil pump pulley
2 | Drive belt
3 | Idler pulley
4 | Generator pulley
5 | Front drive belt auto tensioner
6 | Crankshaft pulley
7 | A/C compressor pulley
8 | Water pump pulley