#
DTC P0711 (ISRAELI SPECS.) [JA5A-EL]

BME050218901207

DTC P0711 | Transaxle fluid temperature (TFT) sensor malfunction (stuck)
--- | ---
DETECTION CONDITION | • If the TFT sensor signal remains outside normal temperature range for 10 min or more, the TCM determines that there is a malfunction. Diagnostic support note: • This is a continuous monitor (CCM). • The MIL illuminates if the TCM detects the above malfunction conditions in two consecutive drive cycles.
• PENDING CODE is available.
• FREEZE FRAME DATA is available.
• The HOLD indicator light does not flash.
• The DTC is stored in the TCM memory.
POSSIBLE CAUSE | • TFT sensor malfunction. • Connector corrosion. • TCM malfunction.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME PID DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related Service Bulletins and/or on-line repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT TFT SENSOR VOLTAGE • Turn the ignition switch to the ON position (engine off). • Is the TCM terminal 1F voltage 1.55 V? | Yes | Go to the next step.
No | Go to Step 6.
4 | VERIFY CURRENT INPUT SIGNAL STATUS - IS CONCERN INTERMITTENT OR CONSTANT? • Start the engine. • Drive the vehicle at 60 km/h {37 mph} or above for 10 min or more.

  - ATF 20 ° C {68 ° F}: 1.55 V
  - ATF 60 ° C {140 ° F}: 0.7 V

• Does the TCM terminal voltage change?
Yes
Go to Step 6.
No | Go to the next step.
5 | INSPECT TERMINAL CONDITION • Turn the ignition switch to the LOCK position. • Disconnect the terminal component No.2 (8-pin). • Inspect the terminals for corrosion. • Are the terminals normal? | Yes | Replace the TFT sensor, then go to the next step.
No | Repair or replace the terminals, then go to the next step.
6 | VERIFY TROUBLESHOOTING OF DTC P0711 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the TCM memory using the WDS or equivalent. • Decrease the ATF temperature to 20 ° C {68 ° F} or below. • Drive the vehicle at 60 km/h {37 mph} or above for 10 min or more.
• Is the same DTC present?
Yes
Replace the TCM, then go to the next step.
(See TCM REMOVAL/INSTALLATION [JA5A-EL].)
No | Go to the next step.
7 | VERIFY AFTER REPAIR PROCEDURE • Perform the "After Repair Procedure". (See AFTER REPAIR PROCEDURE [JA5A-EL].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [JA5A-EL].)
No | DTC troubleshooting completed.