#
VALVE GUIDE REPLACEMENT

A6E242412111E04

## Valve Guide Removal

1. Remove the valve guide from the combustion chamber side using the SST.

## Valve Guide Installation

1. Assemble the SSTs so that depth L is as specified.

  Depth L:
  IN: 12.2-12.8 mm {0.481-0.501 in}
  EX: 12.2-12.8 mm {0.481-0.501 in}

2. Tap the valve guide in from the side opposite the camshaft side until the SSTs contacts the cylinder head.

3. Verify that the valve guide projection height (dimension A ) is within the specification.

  Standard height:
  IN: 12.2-12.8 mm {0.481-0.501 in}
  EX: 12.2-12.8 mm {0.481-0.501 in}