#
AUTOMATIC TRANSAXLE SHIFT MECHANISM STRUCTURAL VIEW

BME051846010T02

General (L.H.D.) specs.

1 | Cannot be engaged unless selector lever is pulled forward
2 | Can be engaged without pulling selector lever forward
3 | Cannot be engaged unless selector lever is pulled forward when brake is depressed
4 | Selector lever
5 | P position switch
6 | Shift-lock solenoid
7 | Key interlock solenoid
8 | Selector cable
9 | Brake switch
10 | Key interlock resistor
11 | Shift-lock relay
12 | Shift-lock release lever

Australian, General (R.H.D.) specs.

1 | Cannot be engaged unless selector lever is pulled forward
2 | Can be engaged without pulling selector lever forward
3 | Cannot be engaged unless selector lever is pulled forward when brake is depressed
4 | Selector lever
5 | P position switch
6 | Shift-lock solenoid
7 | Key interlock solenoid
8 | Selector cable
9 | Brake switch
10 | Key interlock resistor
11 | Shift-lock relay
12 | Shift-lock release lever