#
PID/DATA MONITOR AND RECORD [MZR-CD (RF Turbo)]

BME010200102T11

PID/DATA monitor item table

Monitor item | Unit/Condition | Definition | PCM terminal
--- | --- | --- | ---
ACCS | ON/OFF | Air conditioning compressor cycling switch | 73
ACSW | ON/OFF | A/C request signal. | 84
ACR | ON/OFF | A/C relay | 73
APS1 | V | Accelerator position sensor No.1 - voltage | 10
APS2 | V | Accelerator position sensor No.2 - voltage | 88
ARPMDES | RPM | Target engine speed | -
BARO | Pa | psi | Bar | Barometric pressure | -
V
BOO | ON/OFF | Brake switch | -
BOOST_DSD | Pa | psi | Bar | Desired boost pressure | -
COLP | ON/OFF | Refrigerant pressure switch (middle pressure) | 83
CPP | ON/OFF | Clutch pedal position switch | 33
CPP/PNP | Neutral/Drive | Neutral switch | 56
CR_1 | V | Calibration resistor voltage 1 | 37
CR_2 | V | Calibration resistor voltage 2 | 62
CR_3 | V | Calibration resistor voltage 3 | 89
CR_4 | V | Calibration resistor voltage 4 | 11
DEC_CMP | mm3/Stroke | Desired fuel for torque down control | -
DSC_ACT | Enabled/Disabled | DSC control enable/disable | -
DTCCNT | - | DTC count | -
ECT | °C | °F | Engine coolant temperature | 87
V
EGRA | % | Exhaust gas recirculation solenoid valve (vent) | 72
EGRV | % | Exhaust gas recirculation solenoid valve (vacuum) | 99
EGRV2 | ON/OFF | Exhaust gas recirculation control solenoid valve | 77
FAN_DUTY | ON/OFF | Cooling fan relay No.2 (Main fan relay) | 22
FFH_STAT | Active/Inactive | FFH status | -
FIP_FL | A | FIP flow control | 30
%
FIP_FL_DSD | mm3/Stroke | FIP flow desired | -
FIP_LRN | A | FIP learning amount | -
FIP_MODE | Normal/Fixed_1/Fixed_2/Disabled | FIP duty control status | -
FIP_SCV | A | FIP suction control valve | 93, 94
V
FLT | °C | °F | Fuel temperature | 35
FLTV | V | FLT signal voltage | 35
FRP | V | Fuel rail pressure | 61
Pa | psi | Bar
FRP_A | Pa | psi | Bar | FRP after fuel injection | 61
GLWPG V | V | Glow plugs | 86
GPC | ON/OFFf | Glow plug control | 68
IASV | ON/OFF | intake shutter solenoid valve (full) control | 74
IASV2 | ON/OFF | intake shutter solenoid valve (full) control | 100
IAT | V | Intake air temperature | 60
°C | °F
IAT2 | V | Intake air temperature No.2 | 8
°C | °F
ICP | Pa | psi | Bar | Injector control pressure | 33, 56
IMRC | ON/OFF | VSC solenoid valve control | 101
INGEAR | ON/OFF | Load/no load condition | -
INJ_LRN_DIS | m | mile | Distance from the last injector learning | -
INJ_MODE | Normal/Disabled/Spitted/Fixed | Fuel injection timing control status | -
INJ_TIM | ° | Fuel injection timing | 42, 43, 44, 45
INJ1_CMP | mm3/Stroke | Injector 1 correction value | 42
INJ2_CMP | Injector 2 correction value | 45
INJ3_CMP | Injector 3 correction value | 43
INJ4_CMP | Injector 4 correction value | 44
ISC_CMP | mm3/Stroke | Fuel correction for idle speed control | -
IVS | Idle/Off Idle | Idle switch | 31
MAF | g/s | Mass air flow amount | 9
V
MAF_C | g | MAF per cylinder | -
MAF_C_DSD | g | MAF per cylinder desired | -
MAF_LRN_DIS | m | mile | Distance from the last MAF learning | -
MAINRLY | ON/OFF | PCM control relay | 69
MAP | Pa | psi | Bar | Manifold absolute pressure | 36
V
MIL | ON/OFF | Malfunction indicator lamp | 71
MULTI_INJ | 1_INJ/2_INJ/3_INJ/4_INJ/5_INJ/Disabled | Multiple fuel injection control status | -
RPM | RPM | Engine speed | 3, 29
START_SW | ON/OFF | Starter switch value | 57
TC_CMP | mm3/Stroke | Fuel correction when torque down control | -
VBCV | % | VBC solenoid valve control | 67
VFDES | mm3/Stroke | Volume fuel desired | -
VPWR | V | Battery positive voltage | 27, 53, 79
VSS | KPH | MPH | Vehicle speed sensor. | 6