#
RANGE DETERMINATION OPERATION

BME051718880109

• Each range is determined by operating the selector lever, and switching on/off the switch in the TR switch internal circuit. The present range is detected according to the on/off signal of the switch.

• The following switches are built into the TR switch, and determine each range when the switch is on.

P and N position switch

R position switch

D range switch

S range switch

L range switch

• The range is determined to be R when there is no signal from the range switch, and a pre-programmed time has passed.