#
FUEL SYSTEM OUTLINE [AJ]

BME011400000T06
• The fuel system for Mazda MPV has been adopted or changed the following parts.

  - Mechanical returnless fuel system has been adopted.

  • Fuel line pressure has been increased.
  • Pressure regulator has been built in the the fuel pump unit.

  - Fuel tank capacity has been increased to 75 L {19.8 US gal, 16.5 lmp gal}.
  - Quick release connector (fuel tank side) has been changed, that is same as Quick release connector (engine room side).

Item | Remark for new model
--- | ---
Mechanical returnless fuel system | Same function as current MX-5 (NB) BP engine models
Fuel injector | Same function as previous MPV (LW) GY engine models
Pulsation damper | Same function as previous MPV (LW) GY engine models
Quick release connector (fuel distributor side) | Same function as previous MPV (LW) GY engine models
Quick release connector (engine room side) | Same as previous MPV (LW) GY engine models
Quick release connector (fuel tank side) | Same as quick release connector (engine room side) of previous MPV (LW) GY engine models
Fuel tank | Same function as previous MPV (LW) GY engine models Increased fuel tank capacity
Fuel pump unit (built in pressure regulator and fuel filter (high & low pressure)) | Same function as previous MPV (LW) GY engine models pressure regulator has been built in.
Nonreturn valve | Same function as previous MPV (LW) GY engine models