#
KEY INTERLOCK SOLENOID INSPECTION

BME051809000202

## Continuity Inspection

1. Disconnect the negative battery cable.

2. Remove the column cover.

3. Disconnect the key interlock solenoid connector.

4. Inspect for continuity between terminals A and B.

  • If there is any malfunction, replace the key cylinder.

5. Connect the key interlock solenoid connector.

6. Install the column cover.

7. Connect the negative battery cable.