#
DTC B1342 (61)

BME040243000210

DTC | B1342 (61) | ABS/TCS HU/CM (with TCS) or ABS HU/CM (without TCS)
DETECTION CONDITION | The on-board diagnostic function detects computer malfunction.
POSSIBLE CAUSE | • Malfunction of ABS/TCS HU/CM (with TCS) or ABS HU/CM (without TCS)

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY CURRENT STATUS OF MALFUNCTION • Clear DTC from memory. (See Clearing DTCs Procedure) • Start engine and drive vehicle at 10 km/h {6.2 mph} or above. • Is same DTC present? | Yes | Replace ABS/TCS HU/CM (with TCS) or ABS HU/CM (without TCS), then go to next step.
No | Inspect intermittent concern using the same procedure as engine control system. (See INTERMITTENT CONCERN TROUBLESHOOTING [L3]) (See INTERMITTENT CONCERN TROUBLESHOOTING [AJ]) (See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)])
2 | VERIFY AFTER REPAIR PROCEDURE • Is there any other DTC present? | Yes | Go to applicable DTC inspection.
No | Troubleshooting completed.