#
WINDSHIELD WIPER LINK REMOVAL/INSTALLATION

BME091967360201

1. Remove the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

2. Remove the cowl grille. (See COWL GRILLE REMOVAL/INSTALLATION.)

3. Pry off the connection between the windshield wiper motor and windshield wiper link.

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. Adjust the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE ADJUSTMENT.)

1 | Bolt
2 | Windshield wiper link