#
FOREWORD [FN4A-EL]

BME050201030201
• When the customer reports a vehicle malfunction, check the malfunction indicator lamp (MIL), HOLD indicator light flashing, and PCM memory for diagnostic trouble code (DTC), then diagnose the malfunction according to following flowchart.

  - If the DTC exists, diagnose the applicable DTC. (See DTC TABLE [FN4A-EL].)
  - If the DTC does not exist, the MIL does not illuminate, and the HOLD indicator light flashes, diagnose the applicable symptom troubleshooting. (See SYMPTOM TROUBLESHOOTING ITEM TABLE [FN4A-EL].)

*: Malfunction indicator lamp (MIL), HOLD indicator light