#
WHEEL HUB, HUB SPINDLE PRE-INSPECTION

BME031205000W02

## Wheel Bearing Play Inspection

1. Position a dial indicator against the brake drum.

2. Push and pull the rear brake component by hand in the axial direction and measure the wheel bearing play.

  • If the bearing play exceeds the specification, replace and tighten the locknut to the specified torque and retest.
  • Replace the wheel hub component as necessary.

Maximum wheel bearing play

  0.05 mm {0.002 in}