#
DTC P0202 [MZR-CD (RF Turbo)]

BME010200102264

DTC P0202 | Fuel injector No.2 operation identified
--- | ---
DETECTION CONDITION | • The PCM monitors each cylinder injection confirmation signal from the IDM while the engine is running. If the PCM does not receive the injection confirmation signal for No.2 cylinder normally, the PCM determines that the fuel injector No.2 operation is not verified. Diagnostic support note
• The MIL illuminates if the PCM detects the above malfunction condition in the first drive cycle.
• FREEZE FRAME DATA is available.
• The DTC is stored in the PCM memory.
POSSIBLE CAUSE | For the "Type A" and "Type B" specifications explained in the following, refer to "Specification Identification" to identify the service specification. (See SPECIFICATION IDENTIFICATION.) Type A • IDM malfunction • Connector or terminal malfunction
• Short to GND in wiring harness between IDM terminal 2F and PCM terminal 43
• Short to power supply in wiring harness between IDM terminal 2F and PCM terminal 43
• Open circuit in wiring harness between IDM terminal 2F and PCM terminal 43
• Fuel injector No.2 malfunction
• Short to GND in wiring harness between calibration resistor No.2 terminal B and IDM terminal 1G
• Short to power supply in wiring harness between calibration resistor No.2 terminal B and IDM terminal 1G
• Open circuit in wiring harness between calibration resistor No.2 terminal B and IDM terminal 1G
• PCM malfunction
Type B
• IDM malfunction
• Connector or terminal malfunction
• Short to GND in wiring harness between IDM terminal 2F and PCM terminal 43
• Short to power supply in wiring harness between IDM terminal 2F and PCM terminal 43
• Open circuit in wiring harness between IDM terminal 2F and PCM terminal 43
• Fuel injector No.2 malfunction
• Short to GND in wiring harness between fuel injector No.2 terminal B and IDM terminal 1G
• Short to power supply in wiring harness between fuel injector No.2 terminal B and IDM terminal 1G
• Open circuit in wiring harness between fuel injector No.2 terminal B and IDM terminal 1G
• PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related Service Bulletins and/or on-line repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY CURRENT SIGNAL STATUS: IS CONCERN INTERMITTENT OR CONSTANT? • Connect the WDS or equivalent to the DLC-2. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Go to the next step.
No | Intermittent concern exists. Perform the "INTERMITTENT CONCERN TROUBLESHOOTING". (See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)].)
4 | IDENTIFY TRIGGER DTC FOR FREEZE FRAME DATA • Is DTC P0202 on FREEZE FRAME DATA? | Yes | Go to the next step.
No | Go to the troubleshooting procedures for the DTC in the FREEZE FRAME DATA.
5 | INSPECT IDM CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Inspect for poor connection (such as damaged/pulled-out terminals, corrosion). • Is there any malfunction? | Yes | Repair or replace the suspected terminal, then go to Step 14.
No | Go to the next step.
6 | INSPECT IDM FOR SHORT TO GND • Turn the engine switch off. • Inspect the continuity between the following terminals and body GND.

  - IDM terminal 2F (wiring harness-side)
  - IDM terminal 1G (wiring harness-side)

• Is there continuity?
Yes
Repair or replace the wiring harness for a short to GND, then go to Step 14.
No | Go to the next step.
7 | INSPECT IDM FOR SHORT TO POWER • Turn the engine switch to the ON position (Engine off). • Inspect the voltage between the following terminals and body GND.

  - IDM terminal 2F (wiring harness-side)
  - IDM terminal 1G (wiring harness-side)

• Is the voltage B+?
Yes
Repair or replace the wiring harness for a short to power supply, then go to Step 14.
No | Go to the next step.
8 | INSPECT FUEL INJECTOR NO.2 CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Inspect for poor connection (such as damaged/pulled-out terminals, corrosion). • Is there any malfunction? | Yes | Repair or replace the suspected terminal, then go to Step 14.
No | Go to the next step.
9 | INSPECT FOR OPEN CIRCUIT BETWEEN IDM AND FUEL INJECTOR NO.2 • Turn the engine switch off. • Inspect for continuity between the following terminals: Type A

  - IDM terminal 1G (wiring harness-side) and calibration resistor No.2 terminal B (wiring harness-side).

Type B

  - IDM terminal 1G (wiring harness-side) and fuel injector No.2 terminal B (wiring harness-side).

• Is there continuity?
Yes
Go to the next step.
No | Repair or replace the wiring harness for an open circuit then go to Step 14.
10 | INSPECT FUEL INJECTOR • Inspect the fuel injector No.2. (See FUEL INJECTOR INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace fuel injector No.2, then go to Step 14.
No | Go to the next step.
11 | INSPECT IDM • Inspect the IDM. (See INJECTOR DRIVER MODULE (IDM) INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace the IDM, then go to step 14.
No | Go to the next step.
12 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Inspect for poor connection (such as damaged/pulled-out terminals, corrosion). • Is there any malfunction? | Yes | Repair or replace the suspected terminal, then go to Step 14.
No | Go to the next step.
13 | INSPECT FOR OPEN CIRCUIT BETWEEN IDM AND PCM • Turn the engine switch off. • Inspect the continuity between IDM terminal 2F (wiring harness-side) and PCM terminal 43 (wiring harness-side). • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for an open circuit, then go to the next step.
14 | VERIFY TROUBLESHOOTING OF DTC P0202 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Replace the PCM, then go to the next step.
No | Go to the next step.
15 | VERIFY AFTER REPAIR PROCEDURE • Perform the Repair Verification Drive Mode. (See OBD DRIVE MODE [MZR-CD (RF Turbo)].) • Are any DTCs present? | Yes | Go to the applicable DTC troubleshooting. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | Troubleshooting completed.