#
BATTERY RECHARGING

BME011718520204

  Caution

  • To avoid damaging the battery, do not quick charge for over 30 min.

1. Remove the battery from vehicle and place it in a pan of water.

2. Connect a battery charger to the battery.

3. Adjust the charging current as follows.

Battery type (5-h rate) | Slow charge (A) | Quick charge (A)
--- | --- | ---
55D23L (48) | 4.5-5.5 | 30
80D26L (55) | 5.5-6.5 | 35
95D31L (64) | 6.5-8.0 | 40
115D31L (70) | 7.0-8.5 | 45

4. After the battery has been recharged, measure the battery positive voltage and verify that the battery keeps specified voltage for more than 1 h.

  • If it exceeds the specification, replace the battery.

Standard

  12.4 V or more