#
LIFTGATE LOWER TRIM REMOVAL/INSTALLATION

BME091768960201

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim.

3. Remove the liftgate side trim.

4. Remove the cargo compartment light. (See CARGO COMPARTMENT LIGHT REMOVAL/INSTALLATION.)

5. Remove the liftgate lower trim installation fasteners.

6. Remove the pull handle installation screws.

7. Remove the pull handle.

8. Pull the liftgate lower trim forward to disengage clips A and pins B from the body, and remove the liftgate lower trim.

9. Install in the reverse order of removal.